****

**Commercial fire/burglary multitasking, multiplexing, partitioning control**

**MA3000**

* **12 - 96 Fully programmable zones (8 zones on board + 4 at each RP3000LCD keypad)  
  8 Partitions**
* **8 Doors built-in access control**
* **96 Simplified multi-function, multi-level user codes**
* **800 Event history log**
* **8 to 64 Prog. relays**
* **Real time clock & 255 event scheduler**
* **Expandable with EZM3008 8-zone multiplex modules**
* **On-site parallel printer output**
* **Advanced false alarm prevention features for extra-simple user operation**

**Accessories:**

* **Housings - standard H1214, commercial H1518 or commercial fire CF1518 EZM3008 8 zone multiplex module**
* **RB3008 8-Relay board , CF5530 commercial fire module**
* **RP3000LCDe dual line alpha burglar/fire/access keypad with 4 built-in zones**
* **CF3000LCDe dual line alpha Fire Marshall keypad with 4 built-in zones**
* **PS3000 Heavy duty 4A power supply**

**MA1000ENB Control**

* **7 EOL + N/O zones**
* **Supervised fire zone  
  up/downloadable full-size control w/ 45° terminal strip**
* **8 user codes  
  transformer supplied  
  High-economy MA1000E also available, as above with large cabinet**
* **Uses matching RP1000eLCD**
* **Alpha keypad and digital RP1054e keypad models**

**MA1008ENB Control**

* **8 EOL + n/o zones**
* **2-Wire supervised fire zone  
  180 Event time-referenced history log**
* **Powerful built-in siren driver**
* **Up/downloadable full-size control w/ full-size terminal strip**
* **8 User codes**
* **Uses matching RP1000eLCD alpha keypad and digital RP1054e keypad models**



**Backlit digital display keypad**

**RP1054E/RP1016E**

* **3 F-P-A (fire, panic, auxiliary) Panic keys**
* **Backlit touchtone keys**
* **Vivid digital display + status LEDs**



**Backlit custom alphanumeric keypad**

**RP1000ELCD  
as above, but with:**

* **Large, backlit custom English language display & alpha zone directory**
* **Backlit touchtone keys auto-brighten at a touch**



**Burglar/Fire/Access control backlit custom alphanumeric scroll keypad**

**RP3000LCD**

Large, backlit custom English language display & alpha zone directory  
Easier than ever usage  
3 F-P-A panics  
Backlit touchtone keys auto-brighten with a touch  
4-EOL zone built-in multiplex module at each keypad  
• Supervised tamper  
• 3-in-1 Keypad: Simultaneous use as arm/disarm station, burglary system control and access control entry point  
• Guard tour option