**ContactUs asto e.g. info disclosure on e.g. what is needed in order to propose you a sustainable & suitable taylormake quote e.g.Meterings /borehole depth,actual head fitness strenght,static/dynamic level heads,water per day/s;tested/certified/dates /@diverse intervals,winters/summers,recoveries/reverse rate/s...,overhourly maxes,horizontal pumping etc AS WELL AS E.G.tank/irrigations/sprinklings/drippings/related,various eg capacities/ various heads/temperatures//different uses/baffles/ various pip/es/ thicknesses /frequency shiftings, multi-staged couplings/all losses/ sleeved /location &gpscordinates/consentrated/ recovery rates & balances/ condensed levelling/bar suctionsgradient/solar arrays, yields/ auto soft starts..., monthly usage/s/costs,various "standing"etc waterlevels,cusecs/feets,nonreturn valves/ related expansions/ /gallons/ well points/ friction losses/ boost v/ geological cards /transverabilities /gps locations, bidems, profiling, cleanings, frictions, age...of borehole/when e.g.drilled/previous problems/related etc. (These type/s of aspects normally apply to all sorts of pumps 220 volts etc aswell). ContactUS 4QUALITY assistance on e.g.formal qualified borehole certificated testing etc doneby outside consultancy (not always available). Please read SMG terms concerning knowledge provided on their sites, & all quote/s&/designing requests etc. If eg *SM recommended installers not utilized, these may affect warranties, concerning all SM/G products aswell as systems.***